/** \file
 *
 *  This file contains special DoxyGen information for the generation of the main page and other special
 *  documentation pages. It is not a project source file.
 */

/** \page Page_CompilingApps Compiling the Demos, Bootloaders and Projects
 *
 *  The following details how to compile the included LUFA demos, applications and bootloaders using AVR-GCC.
 *
 *  \section Sec_Prerequisites Prerequisites
 *  Before you can compile any of the LUFA library code or demos, you will need a recent distribution of avr-libc (1.6.2+)
 *  and the AVR-GCC (4.2+) compiler. A standard "coreutils" package for your system is also required for command line
 *  compilation of LUFA based applications.
 *
 *  \subsection SSec_PreqWindows Windows Prerequisites
 *  On Windows, you will need a copy of the latest Atmel Toolchain (<a>http://www.atmel.com/tools/ATMELAVRTOOLCHAINFORWINDOWS.aspx</a>),
 *  either downloaded and installed as a standalone package, or installed as part of Atmel Studio. You will need to ensure
 *  that the "bin" directory of the toolchain is available in your system's <b>PATH</b> environment variable.
 *
 *  In addition, you will need to install a ported version of the ZSH or BASH *nix shells, and a standard set of *nix
 *  utilities such as <i>cut</i>, <i>find</i> and <i>sed</i>. These can be found in the "basic" system package of the
 *  of the MinGW installer (<a>http://www.mingw.org</a>). Once installed, add the "msys\1.0\bin" of the MinGW installation
 *  folder is added to your system's <b>PATH</b> environment variable.
 *
 *  \subsection SSec_PreqLinux Linux Prerequisites
 *  On Linux systems you will need to install the latest Linux distribution of the standalone Atmel Toolchain from the
 *  Atmel website (<a>http://www.atmel.com/tools/ATMELAVRTOOLCHAINFORLINUX.aspx</a>), or use the latest avr-libc and avr-gcc packages
 *  for your chosen distribution's package manager. For full device support, the Atmel standalone Toolchain package is recommended.
 *
 *  \section Sec_Compiling Compiling a LUFA Application
 *  Compiling the LUFA demos, applications and/or bootloaders is very simple. LUFA comes with makefile scripts for
 *  each individual demo, bootloader and project folder, as well as scripts in the Demos/, Bootloaders/, Projects/
 *  and the LUFA root directory. Compilation of projects can be started from any of the above directories, with a build
 *  started from an upper directory in the directory structure executing build of all child directories under it. This
 *  means that while a build inside a particular demo directory will build only that particular demo, a build started from
 *  the /Demos/ directory will build all LUFA demo projects sequentially.
 *
 *  To build a project from the source via the command line, the command <b>"make all"</b> should be executed from the command
 *  line in the directory of interest. To remove compiled files (including the binary output, all intermediately files and all
 *  diagnostic output files), execute <b>"make clean"</b>. Once a "make all" has been run and no errors were encountered, the
 *  resulting binary will be located in the generated ".HEX" file. If your project makes use of pre-initialized EEPROM
 *  variables, the generated ".EEP" file will contain the project's EEPROM data.
 *
 *  \see \ref Page_BuildSystem for information on the LUFA build system.
 */
